Do now:

1. Binary is base 2
2. Denary is base 10
3. Hex is base 16
4. An OR gate is a logic gate which requires one input to be 1 for the output to be 1